Quick-Start guide firmware flashing to C5 Hardware and OpenXC Firmware

Rev 3

Windows:

1. Download OpenXC installation package [here](http://vi-firmware.openxcplatform.com/en/master/_static/OpenXC-CrossChasm-Flash.zip).
2. Create a folder on your computer and extract the package.
3. Put the hex file that you want to flash in this new folder as well. You can [build your own](http://openxcplatform.com/firmware/advanced-intro.html) firmware or obtain one for [supported vehicles](http://openxcplatform.com/hardware/vehicles.html).
4. Copy "libusb0.dll" to c:\Windows\SysWOW64 for 64-bit Windows, or c:\Windows\system32 for 32-bit Windows
5. Copy "libusb0.sys" to c:\Windows\system32\drivers
6. Connect the C5 to your computer via USB cable, the USB bootloader will run for about 5 seconds (blinking red and solid blue lights).
7. While the USB bootloader is running (first 5 seconds after power-up), use Device Manager to manually install the provided driver file "stk500v2.inf" (note that Windows 8 will indicate the file has not been signed – ignore this message).
8. Open a command prompt window and navigate to the folder that you created in step number 2.
9. Disconnect and re-connect the OpenXC device.
10. Within 5 seconds of connecting the device, run avrdude using "avrdude.exe -U flash:w:<HEX> -c stk500 -p 32MX795F512L -C avrdude.conf -P COM<n>", where <HEX> is the name of your firmware file (that you copied into the folder) and <n> is the com port number for the OpenXC device (you can use Device Manager to check this).
11. After flashing is complete, power cycle the device and initialize the [RTC](http://vi-firmware.openxcplatform.com/en/master/advanced/rtc.html) via the Python command ($ openxc-control set --time 1461545558), but using the [current UNIX time](http://www.unixtimestamp.com/).
12. Enjoy!

MAC / Linux:

1. Download OpenXC installation package [here](http://vi-firmware.openxcplatform.com/en/master/_static/OpenXC-CrossChasm-Flash.zip).
2. Create a folder on your computer and extract the package.
3. Put the hex file that you want to flash in this new folder as well. You can [build your own](http://openxcplatform.com/firmware/advanced-intro.html) firmware or obtain one for [supported vehicles](http://openxcplatform.com/hardware/vehicles.html).
4. Connect the C5 to your computer via USB cable, the USB bootloader will run for about 5 seconds (blinking red and solid blue lights).
5. Open a command line window and identify which device is plugged in by searching through the output of “$ ls /dev/tty.usb\*” The device should appear as something similar to /dev/tty.usbmodem1421.
6. Disconnect and re-connect the OpenXC device.
7. Within 5 seconds of connecting the device, run avrdude using "./avrdude\_mac -U flash:w:<HEX> -c stk500 -p 32MX795F512L -C avrdude.conf -P <id>", where <HEX> is the name of your firmware file (that you copied into the folder) and <id> is the OpenXC device such as “/dev/tty.usbmodem1421”.
8. After flashing is complete, power cycle the device and initialize the [RTC](http://vi-firmware.openxcplatform.com/en/master/advanced/rtc.html) via the Python command ($ openxc-control set --time 1461545558), but using the [current UNIX time](http://www.unixtimestamp.com/).
9. Enjoy!